(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Oscillator_100MHz_SG3225EEN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Oscillator_100MHz_SG3225EEN"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Oscillator_100MHz_SG3225EEN"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG3225EEN&lang=en"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "100 MHz XO (Standard) LVPECL Oscillator 3.3V Enable/Disable 6-SMD, No Lead"
				(at 20.32 -33.02 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "100MHz"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "MPN" "SG3225EEN_100.000000M-CJGA3"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Epson"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "OSCILLATOR, LVDS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Oscillator_100MHz_SG3225EEN_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin no_connect line
					(at 16.51 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT+")
					(number "4")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "OUT-")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
