(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Choke_SRF2012A-801Y"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "T"
				(at 17.78 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Choke_SRF2012A-801Y"
				(at 17.78 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Choke_SRF2012A-801Y"
				(at 17.78 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.bourns.com/docs/product-datasheets/srf2012a-801y.pdf"
				(at 17.78 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "2 Line Common Mode Choke Surface Mount 800 Ohms @ 100 MHz 300mA DCR 880mOhm"
				(at 17.78 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Bourns"
				(at 17.78 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SRF2012A-801Y"
				(at 17.78 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "IMax" "0.3 A"
				(at 17.78 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 17.78 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 17.78 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CHOKE, PASSIVE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "IND_ACM9070_TDK"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Choke_SRF2012A-801Y_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 10.16 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 10.16 -5.08 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "4")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
