(footprint "antmicro_srp2510tma_r22m"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "L_1008_2520Metric::bourns replacement land pattern per manufacturer datasheet: Bourns SRP2510TMA datasheet p.1 Recommended Layout: overall 2.9, pad 1.2x2.3, gap 0.5")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.6) (layer "F.SilkS"))
  (fp_text value "VAL**" (at 0 2.6) (layer "F.Fab"))
  (pad "1" smd rect (at -0.85 0) (size 1.2 2.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0.85 0) (size 1.2 2.3) (layers "F.Cu" "F.Paste" "F.Mask"))
)
