(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "L_4u7_1.55A_Bourns-SRP2512A"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "L"
				(at 15.24 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "L_4u7_1.55A_Bourns-SRP2512A"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "L_4u7_1.55A_Bourns-SRP2512A"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/srp2512a.pdf"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4.7 µH Shielded Drum Core, Wirewound Inductor 1.55 A 235mOhm Max 1008 (2520 Metric)"
				(at 15.24 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "4u7/1.55A"
				(at 15.24 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bourns"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SRP2512A-4R7M"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ISat" "1.9 A"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "IMax" "1.55 A"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Size" "2.5x2.0"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "L_4u7_1.55A_Bourns-SRP2512A_0_1")
			(symbol "L_4u7_1.55A_Bourns-SRP2512A_1_1"
				(pin passive line
					(at 0 0 0)
					(length 0.508)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 0.508)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
