(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "C_Pol_330u_2.5V_KEMET-T598-D"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "C"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "C_Pol_330u_2.5V_KEMET-T598-D"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "C_Pol_330u_2.5V_KEMET-T598-D"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/447/KEM_T2073_T59X-3700828.pdf"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Tantalum Polymer Capacitor, 330 µF, ± 20%, 2.5 V, ESR 6 mOhm, 1411 [3528 Metric], -55C/+125C"
				(at 18.288 -34.544 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "T598D337M2R5ATE006"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "KEMET"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "330u"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Voltage" "2.5V"
				(at 15.24 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Dielectric" "TA2O5"
				(at 18.288 -32.004 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "C_Pol_330u_2.5V_KEMET-T598-D_0_1")
			(symbol "C_Pol_330u_2.5V_KEMET-T598-D_1_1"
				(pin passive line
					(at 0 0 0)
					(length 1.8542)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 1.8542)
					(name "")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
)
