(footprint "antmicro_tfm252012alma2r2mtaa"
  (version 20240108) (generator "partreel")
  (layer "F.Cu")
  (descr "L_1008_2520Metric::tdk replacement land pattern per manufacturer datasheet: TDK TFM252012ALMA catalog (20200823) p.3 recommended land pattern: pad 0.7x2.0, gap 1.5 (matches 0.6mm terminals)")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.45) (layer "F.SilkS"))
  (fp_text value "VAL**" (at 0 2.45) (layer "F.Fab"))
  (pad "1" smd rect (at -1.1 0) (size 0.7 2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 1.1 0) (size 0.7 2) (layers "F.Cu" "F.Paste" "F.Mask"))
)
