(footprint "Texas_VSON-14-1EP_3x4x1mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "DSJ (R-PVSON-N14)")
	(tags "Integrated Circuit")
	(property "Reference" "REF**"
		(at 0 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_VSON-14-1EP_3x4x1mm_P0.5mm"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -2.1 5.9 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.1 7.1 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2 4.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -1.4 -1.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -1.4 -1 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -1.4 -0.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -1.4 0 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -1.4 0.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -1.4 1 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -1.4 1.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at 1.4 1.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at 1.4 1 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at 1.4 0.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at 1.4 0 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at 1.4 -0.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at 1.4 -1 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at 1.4 -1.5 270)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.69 -1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.69 1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.23 -1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.23 1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0 0)
		(size 1.58 2.85)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at 0.23 -1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0.23 1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0.69 -1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 0.69 1.815)
		(size 0.2 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_tps63020qdsjrq1.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
