(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Resonator_38.4MHz_TZ3398B"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "Y"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Resonator_38.4MHz_TZ3398B"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Resonator_38.4MHz_TZ3398B"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.taisaw.com/assets/PDF/TZ3398B%20_Rev.4.0_.pdf"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Crystal, 38.4 MHz ±10ppm 10pF 40 Ohms 4-SMD, No Lead"
				(at 15.24 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TZ3398B"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TST"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Val" "38.4 MHz"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, CERAMIC, OSCILLATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Resonator_38.4MHz_TZ3398B_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 3.81 -5.08 90)
					(length 2.54)
					(name "SH")
					(number "2")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 3.81 -5.08 90)
					(length 2.54)
					(hide yes)
					(name "SH")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
