(footprint "R_Shunt_Vishay_WSK2512"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "R_Shunt_Vishay_WSK2512"
		(at 0 2.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.7 3.841 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.7 5.041 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.7 6.241 0)
		(layer "F.Fab")
	)
	(pad "I1" smd rect
		(at -1.715 -0.635)
		(size 3.175 2.032)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0254)
	)
	(pad "I2" smd rect
		(at 1.715 0.635)
		(size 3.175 2.032)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.0254)
	)
	(pad "V1" smd rect
		(at -2.605 1.27)
		(size 1.397 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "V2" smd rect
		(at 2.605 -1.27)
		(size 1.397 0.762)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(embedded_fonts no)
	(model "antmicro_wsk25121l000fea.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -180)
		)
	)
)
