(footprint "CAPC1320X95N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor, Non-Polarized,Chip 0508 1220;1.25mm L X 2.00mm W X 0.95mm H, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -1.96 0)
		(layer "F.SilkS")
	)
	(property "Value" "CAPC1320X95N"
		(at 0 1.96 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.56 0 90)
		(size 2.14 0.67)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.56 0 90)
		(size 2.14 0.67)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
