(footprint "FIL_MURATA_BNX016"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Block Type EMIFIL LC Combined Type, BNX01* Series")
	(property "Reference" "REF**"
		(at 0 -6.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "FIL_MURATA_BNX016"
		(at 0 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "CG"
		(at -3.50001 5.247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CG"
		(at 1.4 0.747 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "B"
		(at 2.2 -3.753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "PSG"
		(at -4 -3.753 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "CB"
		(at 1.5 5.247 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at 2.5 -2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 2.5 2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -2.5 -2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -2.5 2.5)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 0 0)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 5 0)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
