(footprint "FIL_SCHURTER_FPP-01(13P)"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0.6 to 6.5A 250VAC Single Phase Low Cost PCB Filter (Body 45 x 28x 16.5mm)")
	(property "Reference" "REF**"
		(at 0.00019 -13.30019 0)
		(layer "F.SilkS")
	)
	(property "Value" "FIL_SCHURTER_FPP-01(13P)"
		(at 0.00019 13.29983 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "E" thru_hole circle
		(at 0.00019 -7.50019 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L" thru_hole circle
		(at 10.0002 9.99982 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L'" thru_hole circle
		(at -9.99982 9.99982 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "N" thru_hole circle
		(at 10.0002 -5.00019 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "N'" thru_hole circle
		(at -9.99982 -5.00019 180)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
