(footprint "INDC2012X105N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Inductor, EIA 0805, Metric 2012, Body 2.0x1.25mm, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -1.725 0)
		(layer "F.SilkS")
	)
	(property "Value" "INDC2012X105N"
		(at 0 1.725 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.9 0 90)
		(size 1.45 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.9 0 90)
		(size 1.45 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
