(footprint "IND_MURATA_BLM31PG"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Ferrite Bead, 3.20mm L X 1.60mm W, BLM31PG Series")
	(property "Reference" "REF**"
		(at 0.000045 -1.875 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_MURATA_BLM31PG"
		(at 0.000045 1.875 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -1.67496 0)
		(size 1.35 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.67504 0)
		(size 1.35 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
