(footprint "IND_MURATA_NFZ32BW"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD EMI Suppression Chip Ferrite Bead (NFZ32BW Series)")
	(property "Reference" "REF**"
		(at -0.00008 -2.37492 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_MURATA_NFZ32BW"
		(at -0.00008 2.37508 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -1.25008 0.00008)
		(size 1.65 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.24992 0.00008)
		(size 1.65 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
