(footprint "INDC4532X170N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Chip;  4.50mm L X 3.20mm W X 1.70mm H, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -2.675 0)
		(layer "F.SilkS")
	)
	(property "Value" "INDC4532X170N"
		(at 0 2.675 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.1 0 90)
		(size 3.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.1 0 90)
		(size 3.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
