(footprint "IND_CERN_HCRAPQU001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HF Common Mode Inductor")
	(property "Reference" "REF**"
		(at 0 -25.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_CERN_HCRAPQU001"
		(at 0 25.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at 13.33334 -22.06626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 13.28572 23.93376 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -14.23811 -22.06626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -14.66668 23.93376 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "" np_thru_hole circle
		(at 0 -21)
		(size 1 1)
		(drill 5.5)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 2.25)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 0 -8.5)
		(size 1 1)
		(drill 5.5)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 2.25)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 0 8.5)
		(size 1 1)
		(drill 5.5)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 2.25)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 0 21)
		(size 1 1)
		(drill 5.5)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 2.25)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at -10 -23)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -10 23)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 10 -23)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 10 23)
		(size 3.2 3.2)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
