(footprint "IND_MURATA_DLW5BT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Common Mode Choke Coil/Noise Filter, DLW5BT Series, Body 5.3 x 5.3mm")
	(property "Reference" "REF**"
		(at 0.00008 -3.975 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_MURATA_DLW5BT"
		(at 0.00008 3.625 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -1.9 1.36125 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -2.1 -0.73875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at 1.8 -0.73875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 1.8 1.36125 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "1" smd rect
		(at -0.94992 1.5)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd custom
		(at -0.44992 0.65)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 1.7) (xy -2.3 1.7) (xy -2.3 1) (xy -1 1) (xy -1 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0.45008 0.65)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 1.7) (xy 2.3 1.7) (xy 2.3 1) (xy 1 1) (xy 1 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at 0.95008 1.5)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd custom
		(at 0.45008 -0.65)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -1.7) (xy 2.3 -1.7) (xy 2.3 -1) (xy 1 -1) (xy 1 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd rect
		(at 0.95008 -1.5)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.94992 -1.5)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd custom
		(at -0.44992 -0.65)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -1.7) (xy -2.3 -1.7) (xy -2.3 -1) (xy -1 -1) (xy -1 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
)
