(footprint "IND_TAIYO-YUDEN_MCF1210"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Inductor Width 1.25mm X Lenght 1mm X Height 0.65mm Body")
	(property "Reference" "REF**"
		(at -0.0875 -1.875 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_TAIYO-YUDEN_MCF1210"
		(at -0.0875 1.575 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.7 -0.275)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.7 0.275)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.7 0.275)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.7 -0.275)
		(size 0.65 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
