(footprint "RES_VISHAY_RTOP200V_FLIP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOT-227B Thick Film Power Resistor")
	(property "Reference" "REF**"
		(at 0.00004 -13.30001 0)
		(layer "F.SilkS")
	)
	(property "Value" "RES_VISHAY_RTOP200V_FLIP"
		(at 0.00004 13.30001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -10.24956 -7.8875)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "1" thru_hole circle
		(at -10.24956 -4.7125)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "1" thru_hole circle
		(at -7.49996 -9.475)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "1" thru_hole roundrect
		(at -7.49996 -6.3)
		(size 9 10.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "1" thru_hole circle
		(at -7.49996 -3.12501)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "1" thru_hole circle
		(at -4.75036 -7.8875)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "1" thru_hole circle
		(at -4.75036 -4.7125)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole circle
		(at 4.75045 4.7125)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole circle
		(at 4.75045 7.8875)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole circle
		(at 7.50005 3.12501)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole roundrect
		(at 7.50005 6.3)
		(size 9 10.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "2" thru_hole circle
		(at 7.50005 9.475)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole circle
		(at 10.24965 4.7125)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(pad "2" thru_hole circle
		(at 10.24965 7.8875)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(tenting none)
	)
	(embedded_fonts no)
)
