(footprint "RN_VISHAY_ACAS0612"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Chip Array, Convex S Version, Pitch 0.80mm, 8-Leads,1.5x3.2mm, VISHAY Type ACAS 0612, IPC Medium Density")
	(property "Reference" "REF**"
		(at -0.2375 -2.565 0)
		(layer "F.SilkS")
	)
	(property "Value" "RN_VISHAY_ACAS0612"
		(at -0.2375 2.565 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.7 -1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.7 -0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.7 0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.7 1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.7 1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.7 0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.7 -0.4)
		(size 0.7 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.7 -1.27)
		(size 0.7 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
