(footprint "RN_VISHAY_CRA12E08"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Chip Array, Pitch 1.27mm, 8 Pin, 3.05mm W X 5.08mm L X 0.70mm H, Serie CRA12E")
	(property "Reference" "REF**"
		(at 0 -3.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "RN_VISHAY_CRA12E08"
		(at 0 3.54 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -1.625 -1.905)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.625 -0.635)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.625 0.635)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.625 1.905)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.625 1.905)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.625 0.635)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.625 -0.635)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.625 -1.905)
		(size 1.05 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
