(footprint "RN_PANASONIC_EXBE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Chip Array, Concave, Pitch 0.80mm, 10 Pin, 2.1mm W X 4.0mm L X 2.3mm H, Type EXBE")
	(property "Reference" "REF**"
		(at 0 -3.57505 0)
		(layer "F.SilkS")
	)
	(property "Value" "RN_PANASONIC_EXBE"
		(at 0 3.57496 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at 0 -2.13755 90)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.1875 -1.20004)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.1875 -0.40004)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.1875 0.39996)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.1875 1.19996)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 2.13746 90)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.1875 1.19996)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.1875 0.39996)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.1875 -0.40004)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.1875 -1.20004)
		(size 0.925 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
