(footprint "VAR_1005X55N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PTC Thermistors, Chip; 3.20mm L X 2.50mm W X 1.80mm H, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0.00008 -1.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "VAR_1005X55N"
		(at 0.00008 1.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -0.54992 0)
		(size 0.45 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.55008 0)
		(size 0.45 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
