(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADAU7118ACPZRL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADAU7118ACPZRL"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADAU7118ACPZRL"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/ADAU7118-1605375.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8-Channel PDM to I2S/TDM Converter, VQFN-16,  Hardware controlable"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADAU7118ACPZRL"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, AUDIO, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADAU7118ACPZRL_1_1"
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PDM_CLK0")
					(number "1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PDM_DAT0")
					(number "2")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PDM_DAT1")
					(number "3")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PDM_CLK1")
					(number "4")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PDM_DAT2")
					(number "5")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "PDM_DAT3")
					(number "6")
				)
				(pin output line
					(at 30.48 -29.21 180)
					(length 2.54)
					(name "SCL")
					(number "7")
				)
				(pin bidirectional line
					(at 30.48 -31.75 180)
					(length 2.54)
					(name "SDA")
					(number "8")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "FSYNC")
					(number "9")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "BCLK")
					(number "10")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "SDATA")
					(number "11")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "ADDR")
					(number "12")
					(alternate "CONFIG" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EN")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDD")
					(number "14")
				)
				(pin power_in line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "IOVDD")
					(number "16")
				)
				(pin power_in line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
