(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADS7828"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADS7828"
				(at 31.75 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADS7828"
				(at 31.75 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7828.pdf"
				(at 31.75 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8 channel12-bit ADC with I2C, 2V7-5V"
				(at 31.75 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADS7828E/250"
				(at 31.75 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 31.75 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 31.75 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONVERTER, IC, ADC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADS7828_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CH0")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CH1")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CH2")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "CH3")
					(number "4")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CH4")
					(number "5")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CH5")
					(number "6")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CH6")
					(number "7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CH7")
					(number "8")
				)
				(pin power_in line
					(at 17.78 -27.94 180)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin bidirectional line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "REF")
					(number "10")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "COM")
					(number "11")
				)
				(pin input line
					(at 17.78 -20.32 180)
					(length 2.54)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at 17.78 -22.86 180)
					(length 2.54)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin bidirectional line
					(at 17.78 0 180)
					(length 2.54)
					(name "SDA")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
