(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADT7476AARQZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADT7476AARQZ"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADT7476AARQZ"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/adt7476a-d.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Remote Thermal Monitor, Fan Controller and Voltage Monitor"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADT7476AARQZ"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Onsemi"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PMIC, SMT, MONITOR, CONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADT7476AARQZ_1_1"
				(pin open_collector line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SDA")
					(number "1")
				)
				(pin open_collector line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "4")
				)
				(pin open_collector line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "GPIO0")
					(number "5")
				)
				(pin open_collector line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "GPIO1")
					(number "6")
				)
				(pin open_collector line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "GPIO2")
					(number "7")
				)
				(pin open_collector line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "GPIO3")
					(number "8")
				)
				(pin input line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "TACH3")
					(number "9")
				)
				(pin open_collector line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "PWM2")
					(number "10")
					(alternate "~{SMB_{ALERT}}" passive line)
				)
				(pin input line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "TACH1")
					(number "11")
				)
				(pin input line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "TACH2")
					(number "12")
				)
				(pin input line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "PWM3")
					(number "13")
					(alternate "~{ADDREN}" passive line)
				)
				(pin input line
					(at 33.02 0 180)
					(length 2.54)
					(name "TACH4")
					(number "14")
					(alternate "GPIO6" passive line)
					(alternate "~{ADDR_{SEL}}" passive line)
				)
				(pin passive line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "D2-")
					(number "15")
				)
				(pin passive line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "D2+")
					(number "16")
				)
				(pin passive line
					(at 33.02 -48.26 180)
					(length 2.54)
					(name "D1-")
					(number "17")
				)
				(pin passive line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "D1+")
					(number "18")
				)
				(pin open_collector line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "GPIO4")
					(number "19")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "+5V_{IN}")
					(number "20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "+12V_{IN}")
					(number "21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "+2.5V_{IN}")
					(number "22")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "V_{CCP}")
					(number "23")
				)
				(pin open_collector line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "PWM1")
					(number "24")
					(alternate "XTO" passive line)
				)
			)
			(embedded_fonts no)
		)
)
