(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BQ24074RGTR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BQ24074RGTR"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BQ24074RGTR"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24074.pdf?ts=1672866260241&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FBQ24074"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Battery Charger with power path,  1 Cell Li-Ion Battery, 1.5A"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BQ24074RGTR"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, MANAGEMENT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BQ24074RGTR_1_1"
				(pin input line
					(at 19.05 -15.24 180)
					(length 2.54)
					(name "TS")
					(number "1")
				)
				(pin passive line
					(at 19.05 -12.7 180)
					(length 2.54)
					(name "BAT")
					(number "2")
				)
				(pin passive line
					(at 19.05 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "BAT")
					(number "3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "~{CE}")
					(number "4")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "EN2")
					(number "5")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "EN1")
					(number "6")
				)
				(pin output line
					(at 19.05 -6.35 180)
					(length 2.54)
					(name "~{PGOOD}")
					(number "7")
				)
				(pin passive line
					(at 19.05 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 19.05 -8.89 180)
					(length 2.54)
					(name "~{CHG}")
					(number "9")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(name "OUT")
					(number "10")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "11")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ILIM")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "13")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TMR")
					(number "14")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ITERM")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ISET")
					(number "16")
				)
				(pin passive line
					(at 19.05 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
