(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BQ25756E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.546 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BQ25756E"
				(at 50.546 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BQ25756E"
				(at 50.546 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/bq25756e"
				(at 50.546 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buck-boost charge controller; 1-7S; Li*, NiMH, SuperCap; Standalone/I²C; Vin 4.2-36V (Vmax 60V)"
				(at 50.546 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 50.546 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BQ25756ERRVR"
				(at 50.546 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.546 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.546 -20.066 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "PMIC, IC, SMT, RoHS, CHARGER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BQ25756E_1_1"
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "SCL")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "SDA")
					(number "2")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 2.54)
					(name "~{INT}")
					(number "3")
				)
				(pin output line
					(at 0 -31.75 0)
					(length 2.54)
					(name "STAT1")
					(number "4")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 2.54)
					(name "STAT2")
					(number "5")
				)
				(pin output line
					(at 0 -29.21 0)
					(length 2.54)
					(name "~{PG}")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 2.54)
					(name "~{CE}")
					(number "7")
				)
				(pin input line
					(at 34.29 -35.56 180)
					(length 2.54)
					(name "TS")
					(number "8")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "ICHG")
					(number "9")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "ILIM_HIZ")
					(number "10")
				)
				(pin input line
					(at 34.29 -33.02 180)
					(length 2.54)
					(name "FBG")
					(number "11")
				)
				(pin input line
					(at 34.29 -30.48 180)
					(length 2.54)
					(name "FB")
					(number "12")
				)
				(pin input line
					(at 34.29 -17.78 180)
					(length 2.54)
					(name "SRN")
					(number "13")
				)
				(pin input line
					(at 34.29 -15.24 180)
					(length 2.54)
					(name "SRP")
					(number "14")
				)
				(pin no_connect line
					(at 31.75 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin no_connect line
					(at 31.75 -24.13 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin power_out line
					(at 34.29 -53.34 180)
					(length 2.54)
					(name "PGND")
					(number "17")
				)
				(pin output line
					(at 34.29 -2.54 180)
					(length 2.54)
					(name "SW2")
					(number "18")
				)
				(pin output line
					(at 34.29 -7.62 180)
					(length 2.54)
					(name "HIDRV2")
					(number "19")
				)
				(pin output line
					(at 34.29 -5.08 180)
					(length 2.54)
					(name "BTST2")
					(number "20")
				)
				(pin output line
					(at 34.29 0 180)
					(length 2.54)
					(name "LODRV2")
					(number "21")
				)
				(pin passive line
					(at 34.29 -53.34 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "22")
				)
				(pin power_in line
					(at 34.29 -44.45 180)
					(length 2.54)
					(name "DRV_SUP")
					(number "23")
				)
				(pin power_out line
					(at 34.29 -41.91 180)
					(length 2.54)
					(name "REGN")
					(number "24")
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "LODRV1")
					(number "25")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "BTST1")
					(number "26")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "HIDRV1")
					(number "27")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SW1")
					(number "28")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ACN")
					(number "29")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ACP")
					(number "30")
				)
				(pin no_connect line
					(at 31.75 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "31")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 2.54)
					(name "VAC")
					(number "32")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "VAC")
					(number "33")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "ACUV")
					(number "34")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "ACOV")
					(number "35")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "FSW_SYNC")
					(number "36")
				)
				(pin power_out line
					(at 34.29 -50.8 180)
					(length 2.54)
					(name "EPAD")
					(number "37")
				)
			)
			(embedded_fonts no)
		)
)
