(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DAC38J84IAAV"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DAC38J84IAAV"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DAC38J84IAAV"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac37j84.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Digital to Analog Converters - DAC Quad-CH 16Bit 1.6/2.5 GSPS"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DAC38J84IAAV"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, SMT, DAC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DAC38J84IAAV_1_1"
				(pin power_in line
					(at 34.29 -38.1 180)
					(length 3.81)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VDDCLK09")
					(number "A8")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VDDCLK09")
					(number "B8")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 3.81)
					(name "VDDAPLL18")
					(number "B9")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "VDDAPLL18")
					(number "B10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C3")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 3.81)
					(name "VDDS18")
					(number "C6")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "VDDS18")
					(number "C7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 3.81)
					(name "LPF")
					(number "C9")
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 3.81)
					(name "VDDAREF18")
					(number "C10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D2")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VDDDIG09")
					(number "D3")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "D4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "D5")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "VQPS18")
					(number "D6")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VQPS18")
					(number "D7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 3.81)
					(name "VDDDAC09")
					(number "D9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDDADAC33")
					(number "D10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "E4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "VDDDAC09")
					(number "E9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDADAC33")
					(number "E10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 3.81)
					(name "VDDR18")
					(number "F2")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VDDT09")
					(number "F3")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "F4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "VDDDAC09")
					(number "F9")
				)
				(pin bidirectional line
					(at 34.29 -30.48 180)
					(length 3.81)
					(name "EXTIO")
					(number "F10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "VDDR18")
					(number "G2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VDDT09")
					(number "G3")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "G4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "VDDDAC09")
					(number "G9")
				)
				(pin output line
					(at 34.29 -33.02 180)
					(length 3.81)
					(name "RBIAS")
					(number "G10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "H4")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H6")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "VDDDAC09")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDADAC33")
					(number "H10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "J4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "J5")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "J6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "VDDDIG09")
					(number "J7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "VDDDAC09")
					(number "J9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDADAC33")
					(number "J10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K2")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "TESTMODE")
					(number "K3")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 3.81)
					(name "VDDIO18")
					(number "K6")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO18")
					(number "K7")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "ATEST")
					(number "K9")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "VDDAREF18")
					(number "K10")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L2")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M4")
				)
				(pin no_connect line
					(at 30.48 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M6")
				)
				(pin no_connect line
					(at 30.48 -19.05 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M7")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M12")
				)
			)
			(symbol "DAC38J84IAAV_2_1"
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "RX6_N")
					(number "A1")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "RX7_N")
					(number "A2")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "RX7_P")
					(number "A3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SYSREF_N")
					(number "A6")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "SYSREF_P")
					(number "A7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DACCLK_N")
					(number "A9")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "DACCLK_P")
					(number "A10")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "RX6_P")
					(number "B1")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SYNCB_N")
					(number "B6")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SYNCB_P")
					(number "B7")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 3.81)
					(name "RX5_P")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 3.81)
					(name "VSENSE")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 3.81)
					(name "IFORCE")
					(number "C5")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "RX5_N")
					(number "D1")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(name "RX4_N")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 3.81)
					(name "AMUX1")
					(number "E3")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 3.81)
					(name "RX4_P")
					(number "F1")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "RX0_P")
					(number "G1")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "RX0_N")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "AMUX0")
					(number "H3")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "RX1_N")
					(number "J1")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "RX1_P")
					(number "K1")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "RX2_P")
					(number "L1")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 3.81)
					(name "SYNC_N_AB")
					(number "L6")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 3.81)
					(name "SYNC_N_CD")
					(number "L7")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "RX2_N")
					(number "M1")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "RX3_N")
					(number "M2")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "RX3_P")
					(number "M3")
				)
			)
			(symbol "DAC38J84IAAV_3_1"
				(pin output line
					(at 34.29 0 180)
					(length 3.81)
					(name "IOUTA_P")
					(number "B12")
				)
				(pin output line
					(at 34.29 -2.54 180)
					(length 3.81)
					(name "IOUTA_N")
					(number "C12")
				)
				(pin output line
					(at 34.29 -7.62 180)
					(length 3.81)
					(name "IOUTB_N")
					(number "D12")
				)
				(pin output line
					(at 34.29 -5.08 180)
					(length 3.81)
					(name "IOUTB_P")
					(number "E12")
				)
				(pin output line
					(at 34.29 -10.16 180)
					(length 3.81)
					(name "IOUTC_P")
					(number "H12")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "TRSTB")
					(number "J3")
				)
				(pin output line
					(at 34.29 -12.7 180)
					(length 3.81)
					(name "IOUTC_N")
					(number "J12")
				)
				(pin output line
					(at 0 -21.59 0)
					(length 3.81)
					(name "TESTMODE")
					(number "K3")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "TCLK")
					(number "K4")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 3.81)
					(name "TXENABLE")
					(number "K5")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 3.81)
					(name "~{RESETB}")
					(number "K8")
				)
				(pin output line
					(at 34.29 -17.78 180)
					(length 3.81)
					(name "IOUTD_N")
					(number "K12")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "TMS")
					(number "L4")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "TDI")
					(number "L5")
				)
				(pin output line
					(at 0 -19.05 0)
					(length 3.81)
					(name "ALARM")
					(number "L8")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "SCLK")
					(number "L9")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "SDIO")
					(number "L10")
				)
				(pin output line
					(at 34.29 -15.24 180)
					(length 3.81)
					(name "IOUTD_P")
					(number "L12")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "TDO")
					(number "M5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 3.81)
					(name "SLEEP")
					(number "M8")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{SDENB}")
					(number "M9")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SDO")
					(number "M10")
				)
			)
			(embedded_fonts no)
		)
)
