(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "INA228AQDGSRQ1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "INA228AQDGSRQ1"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "INA228AQDGSRQ1"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/ina228-q1"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "85V, 20-bit, ultra-precise power/energy/charge monitor with IC interface"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "INA228AQDGSRQ1"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PMIC, SMT, MONITOR, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "INA228AQDGSRQ1_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A1")
					(number "1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A0")
					(number "2")
				)
				(pin open_collector line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "ALERT")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCL")
					(number "5")
				)
				(pin power_in line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "V_{S}")
					(number "6")
				)
				(pin power_in line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{BUS}")
					(number "8")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "IN-")
					(number "9")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "IN+")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
