(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "INA231AIYFFR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 29.21 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "INA231AIYFFR"
				(at 29.21 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "INA231AIYFFR"
				(at 29.21 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina231.pdf?ts=1756752086867&ref_url=https%253A%252F%252Fwww.mouser.dk%252F"
				(at 29.21 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Current-shunt and Power Monitor with 1V8 I2C Interface"
				(at 29.21 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 29.21 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "INA231AIYFFR"
				(at 29.21 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 29.21 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 29.21 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PMIC, SMT, MONITOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "INA231AIYFFR_1_1"
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCL")
					(number "A1")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SDA")
					(number "A2")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 2.54)
					(name "ALERT")
					(number "A3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VS")
					(number "B1")
				)
				(pin no_connect line
					(at 13.97 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B2")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "A0")
					(number "B3")
				)
				(pin power_in line
					(at 16.51 -13.97 180)
					(length 2.54)
					(name "GND")
					(number "C1")
				)
				(pin no_connect line
					(at 13.97 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C2")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "A1")
					(number "C3")
				)
				(pin input line
					(at 16.51 0 180)
					(length 2.54)
					(name "BUS")
					(number "D1")
				)
				(pin input line
					(at 16.51 -8.89 180)
					(length 2.54)
					(name "IN-")
					(number "D2")
				)
				(pin input line
					(at 16.51 -3.81 180)
					(length 2.54)
					(name "IN+")
					(number "D3")
				)
			)
			(embedded_fonts no)
		)
)
