(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IT6251"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IT6251"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IT6251"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://static6.arrow.com/aropdfconversion/985d28c1f7f11650923cfc7afe5edb558f1293c9/it6251.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "High-performance, single-chip De-SSC LVDS to DisplayPort converter"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IT6251"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ITE Tech"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "DISPLAYPORT, LVDS, CONVERTER, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IT6251_1_1"
				(pin no_connect line
					(at 21.59 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 2.54)
					(name "XTALOUT")
					(number "2")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "XTALIN")
					(number "3")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 2.54)
					(name "PVCC2")
					(number "4")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IVDD")
					(number "6")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SYSRSTN")
					(number "7")
				)
				(pin no_connect line
					(at 24.13 0 180)
					(length 2.54)
					(name "DBG0")
					(number "8")
				)
				(pin no_connect line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "DBG1")
					(number "9")
				)
				(pin no_connect line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "DBG2")
					(number "10")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "IVDD")
					(number "11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "OVDD")
					(number "12")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PCADR")
					(number "13")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PCSCL")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PCSDA")
					(number "15")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 2.54)
					(name "ANVDD")
					(number "16")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVCC")
					(number "21")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "ANVDD")
					(number "26")
				)
				(pin power_in line
					(at 24.13 -30.48 180)
					(length 2.54)
					(name "APVDD")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IVDD")
					(number "32")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "ANVDD")
					(number "33")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "AVCC")
					(number "38")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "ANVDD")
					(number "41")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IVDD")
					(number "46")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 2.54)
					(name "AVCC18")
					(number "49")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "AVCC18")
					(number "52")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "AVCC18")
					(number "55")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "AVCC18")
					(number "58")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "AVCC18")
					(number "61")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "REXT")
					(number "62")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 2.54)
					(name "PVCC1")
					(number "63")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "PVCC0")
					(number "64")
				)
				(pin power_in line
					(at 24.13 -33.02 180)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(symbol "IT6251_2_1"
				(pin input line
					(at 25.4 -26.67 180)
					(length 2.54)
					(name "HPD")
					(number "5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RX_A1_N")
					(number "17")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RX_A1_P")
					(number "18")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RX_B1_N")
					(number "19")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RX_B1_P")
					(number "20")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RX_C1_N")
					(number "22")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RX_C1_P")
					(number "23")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RX_CLK_N")
					(number "24")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "RX_CLK_P")
					(number "25")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RX_D1_N")
					(number "27")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RX_D1_P")
					(number "28")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RX_E1_N")
					(number "29")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RX_E1_P")
					(number "30")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "RX_A2_N")
					(number "34")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "RX_A2_P")
					(number "35")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "RX_B2_N")
					(number "36")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "RX_B2_P")
					(number "37")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "RX_C2_N")
					(number "39")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "RX_C2_P")
					(number "40")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "RX_D2_N")
					(number "42")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "RX_D2_P")
					(number "43")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "RX_E2_N")
					(number "44")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "RX_E2_P")
					(number "45")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "TXAUX_N")
					(number "47")
				)
				(pin output line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "TXAUX_P")
					(number "48")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "TX3_N")
					(number "50")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "TX3_P")
					(number "51")
				)
				(pin output line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "TX2_N")
					(number "53")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "TX2_P")
					(number "54")
				)
				(pin output line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "TX1_N")
					(number "56")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "TX1_P")
					(number "57")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "TX0_N")
					(number "59")
				)
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "TX0_P")
					(number "60")
				)
			)
			(embedded_fonts no)
		)
)
