(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT3033EUDC_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT3033EUDC_QFN"
				(at 34.29 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT3033EUDC_QFN"
				(at 34.29 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3033.pdf"
				(at 34.29 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LDO 3A, Vin: 0.95-10V, Vout: 0.2-9.7V, Vdrop: 95mV, Programmable current limit"
				(at 34.29 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT3033EUDC#PBF"
				(at 34.29 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 34.29 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "LDO, POWER, SMT, LINEAR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT3033EUDC_QFN_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "2")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "3")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "4")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ILIM")
					(number "7")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IMON")
					(number "8")
				)
				(pin output line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "REF")
					(number "9")
					(alternate "BYP" passive line)
				)
				(pin input line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "ADJ")
					(number "10")
				)
				(pin output line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "PWRGD")
					(number "11")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "12")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "13")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "15")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "16")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "OUT")
					(number "17")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "18")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "19")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "20")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "22")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "23")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
