(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT3652E_MSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT3652E_MSOP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT3652E_MSOP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.linear.com/docs/28522"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Battery charger"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT3652EMSE#PBF"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, MANAGEMENT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT3652E_MSOP_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN_REG")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "3")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{CHRG}")
					(number "4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{FAULT}")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TIMER")
					(number "6")
				)
				(pin input line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "VFB")
					(number "7")
				)
				(pin input line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "NTC")
					(number "8")
				)
				(pin input line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "BAT")
					(number "9")
				)
				(pin input line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "SENSE")
					(number "10")
				)
				(pin input line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "BOOST")
					(number "11")
				)
				(pin output line
					(at 22.86 0 180)
					(length 2.54)
					(name "SW")
					(number "12")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
