(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT8350RV"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 57.15 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT8350RV"
				(at 57.15 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT8350RV"
				(at 57.15 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt8350.pdf"
				(at 57.15 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 57.15 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT8350RV#PBF"
				(at 57.15 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 57.15 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 57.15 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 57.15 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, POWER, MANAGEMENT, VOLTAGE, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT8350RV_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VIN")
					(number "3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN/UVLO")
					(number "5")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "INTVCC")
					(number "6")
				)
				(pin unspecified line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RP")
					(number "7")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "LOADEN")
					(number "8")
				)
				(pin power_out line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VREF")
					(number "9")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "ISMON")
					(number "10")
				)
				(pin input line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "ISP")
					(number "11")
				)
				(pin input line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "ISN")
					(number "12")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "CTRL")
					(number "13")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "FB")
					(number "14")
				)
				(pin output line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "VC")
					(number "15")
				)
				(pin open_collector line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{PGOOD}")
					(number "16")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SS")
					(number "17")
				)
				(pin input line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "RT")
					(number "18")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "SYNC/MODE")
					(number "19")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "CLKOUT")
					(number "20")
				)
				(pin power_in line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "EXTVCC")
					(number "21")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "LOADTG")
					(number "22")
				)
				(pin power_out line
					(at 25.4 0 180)
					(length 2.54)
					(name "VOUT")
					(number "24")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(hide yes)
					(name "VOUT")
					(number "25")
				)
				(pin output line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "SW2")
					(number "27")
				)
				(pin passive line
					(at 25.4 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "SW2")
					(number "28")
				)
				(pin input line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "BST2")
					(number "29")
				)
				(pin input line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "BST1")
					(number "30")
				)
				(pin output line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "SW1")
					(number "31")
				)
				(pin passive line
					(at 25.4 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "SW1")
					(number "32")
				)
				(pin power_in line
					(at 25.4 -48.26 180)
					(length 2.54)
					(name "GND")
					(number "33")
				)
				(pin passive line
					(at 25.4 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "34")
				)
				(pin passive line
					(at 25.4 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "35")
				)
				(pin passive line
					(at 25.4 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "36")
				)
				(pin passive line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
