(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT9611"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT9611"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT9611"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.lontiumsemi.com/UploadFiles/2021-09/LT9611_Brief_R1.pdf"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "2-Port MIPI to HDMI1.4 Converter, dual-port MIPI® D-PHY receiver, 4 data lanes (2Gbps), 16Gbs max input bandwidth"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT9611"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lontium"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT9611_1_1"
				(pin unspecified line
					(at 33.02 -96.52 180)
					(length 2.54)
					(name "M0_N2")
					(number "1")
				)
				(pin unspecified line
					(at 33.02 -99.06 180)
					(length 2.54)
					(name "M0_P2")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC33_MRX01")
					(number "3")
				)
				(pin power_in line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "VCC12_MRX01")
					(number "4")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "M3_N0")
					(number "5")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "M3_P0")
					(number "6")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "M2_N0")
					(number "7")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "M2_P0")
					(number "8")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "MC_N0")
					(number "9")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "MC_P0")
					(number "10")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "M1_N0")
					(number "11")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "M1_P0")
					(number "12")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 2.54)
					(name "M0_N0")
					(number "13")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 2.54)
					(name "M0_P0")
					(number "14")
				)
				(pin power_in line
					(at 33.02 0 180)
					(length 2.54)
					(name "VDD1")
					(number "15")
				)
				(pin power_in line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "VDD2")
					(number "16")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "RST_N")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "CSCL_GPIO10")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "CSDA_GPIO11")
					(number "19")
				)
				(pin bidirectional line
					(at 33.02 -66.04 180)
					(length 2.54)
					(name "SPI_CSN")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 2.54)
					(name "SPI_MISO")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -71.12 180)
					(length 2.54)
					(name "GPIO4")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "INTIO_GPIO5")
					(number "23")
				)
				(pin bidirectional line
					(at 33.02 -53.34 180)
					(length 2.54)
					(name "CEC_GPIO6")
					(number "24")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 2.54)
					(name "I2C_ADDR")
					(number "25")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "VC33_IO")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 2.54)
					(name "I2S_WS_GPIO7")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 2.54)
					(name "I2S_SCLK_GPIO8")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 2.54)
					(name "I2S_MCLK_GPIO9")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 2.54)
					(name "I2S_D0_SPDIF")
					(number "30")
				)
				(pin power_in line
					(at 33.02 -6.35 180)
					(length 2.54)
					(name "VDD3")
					(number "31")
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 2.54)
					(name "SPI_MOSI")
					(number "32")
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 2.54)
					(name "SPI_SCK")
					(number "33")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 2.54)
					(name "VCC33_IO")
					(number "34")
				)
				(pin input line
					(at 33.02 -55.88 180)
					(length 2.54)
					(name "HTX_HPD")
					(number "35")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "HTX_DSDA")
					(number "36")
				)
				(pin output line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "HTX_DSCL")
					(number "37")
				)
				(pin output line
					(at 33.02 -50.8 180)
					(length 2.54)
					(name "HTX_C-")
					(number "38")
				)
				(pin output line
					(at 33.02 -48.26 180)
					(length 2.54)
					(name "HTX_C+")
					(number "39")
				)
				(pin output line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "HTX_D0-")
					(number "40")
				)
				(pin output line
					(at 33.02 -43.18 180)
					(length 2.54)
					(name "HTX_D0+")
					(number "41")
				)
				(pin input line
					(at 33.02 -104.14 180)
					(length 2.54)
					(name "VCOM")
					(number "42")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VCC33_HTX")
					(number "43")
				)
				(pin power_in line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "VCC12_HTX")
					(number "44")
				)
				(pin output line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "HTX_D1-")
					(number "45")
				)
				(pin output line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "HTX_D1+")
					(number "46")
				)
				(pin output line
					(at 33.02 -35.56 180)
					(length 2.54)
					(name "HTX_D2-")
					(number "47")
				)
				(pin output line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "HTX_D2+")
					(number "48")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 2.54)
					(name "XTALI")
					(number "49")
				)
				(pin output line
					(at 0 -80.01 0)
					(length 2.54)
					(name "XTALO")
					(number "50")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC33_BG")
					(number "51")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 2.54)
					(name "REXT")
					(number "52")
				)
				(pin power_in line
					(at 33.02 -11.43 180)
					(length 2.54)
					(name "VCC12_SYSPLL")
					(number "53")
				)
				(pin power_in line
					(at 33.02 -8.89 180)
					(length 2.54)
					(name "VDD")
					(number "54")
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 2.54)
					(name "VCC33_MRX23")
					(number "55")
				)
				(pin power_in line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "VCC12_MRX23")
					(number "56")
				)
				(pin input line
					(at 33.02 -76.2 180)
					(length 2.54)
					(name "M3_N2")
					(number "57")
				)
				(pin input line
					(at 33.02 -78.74 180)
					(length 2.54)
					(name "M3_P2")
					(number "58")
				)
				(pin input line
					(at 33.02 -81.28 180)
					(length 2.54)
					(name "M2_N2")
					(number "59")
				)
				(pin input line
					(at 33.02 -83.82 180)
					(length 2.54)
					(name "M2_P2")
					(number "60")
				)
				(pin input line
					(at 33.02 -86.36 180)
					(length 2.54)
					(name "MC_N2")
					(number "61")
				)
				(pin input line
					(at 33.02 -88.9 180)
					(length 2.54)
					(name "MC_P2")
					(number "62")
				)
				(pin input line
					(at 33.02 -91.44 180)
					(length 2.54)
					(name "M1_N2")
					(number "63")
				)
				(pin input line
					(at 33.02 -93.98 180)
					(length 2.54)
					(name "M1_P2")
					(number "64")
				)
				(pin power_in line
					(at 0 -104.14 0)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
