(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTC4020EUHF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTC4020EUHF"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTC4020EUHF"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.linear.com/docs/44025"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "55V Buck-Boost Multi-Chemistry Battery Charger"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTC4020EUHF#PBF"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, MANAGEMENT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTC4020EUHF_1_1"
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TG1")
					(number "1")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "BST1")
					(number "2")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "SGND")
					(number "3")
				)
				(pin power_in line
					(at 0 -66.04 0)
					(length 2.54)
					(name "SENSGND")
					(number "4")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SENSBOT")
					(number "5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SENSTOP")
					(number "6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SENSVIN")
					(number "7")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RT")
					(number "8")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SHDN")
					(number "9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VIN_REG")
					(number "10")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "MODE")
					(number "11")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "STAT1")
					(number "12")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "STAT2")
					(number "13")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "TIMER")
					(number "14")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 2.54)
					(name "RNG/SS")
					(number "15")
				)
				(pin input line
					(at 27.94 -76.2 180)
					(length 2.54)
					(name "NTC")
					(number "16")
				)
				(pin input line
					(at 27.94 -73.66 180)
					(length 2.54)
					(name "VFB")
					(number "17")
				)
				(pin input line
					(at 27.94 -71.12 180)
					(length 2.54)
					(name "FBG")
					(number "18")
				)
				(pin input line
					(at 27.94 -68.58 180)
					(length 2.54)
					(name "VFBMIN")
					(number "19")
				)
				(pin input line
					(at 27.94 -66.04 180)
					(length 2.54)
					(name "BAT")
					(number "20")
				)
				(pin output line
					(at 27.94 -60.96 180)
					(length 2.54)
					(name "BGATE")
					(number "21")
				)
				(pin input line
					(at 27.94 -55.88 180)
					(length 2.54)
					(name "CSN")
					(number "22")
				)
				(pin input line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "CSP")
					(number "23")
				)
				(pin output line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "CSOUT")
					(number "24")
				)
				(pin input line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "ILIMIT")
					(number "25")
				)
				(pin input line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "VFBMAX")
					(number "26")
				)
				(pin input line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "ITH")
					(number "27")
				)
				(pin input line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "VC")
					(number "28")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 2.54)
					(name "SGND")
					(number "29")
				)
				(pin power_out line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "BST2")
					(number "30")
				)
				(pin output line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "TG2")
					(number "31")
				)
				(pin input line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "SW2")
					(number "32")
				)
				(pin output line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "BG2")
					(number "33")
				)
				(pin power_out line
					(at 27.94 0 180)
					(length 2.54)
					(name "INTVCC")
					(number "34")
				)
				(pin power_in line
					(at 0 -76.2 0)
					(length 2.54)
					(name "PGND")
					(number "35")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PVIN")
					(number "36")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "BG1")
					(number "37")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SW1")
					(number "38")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "SGND")
					(number "39")
				)
			)
			(embedded_fonts no)
		)
)
