(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX17260_TDFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX17260_TDFN"
				(at 35.56 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX17260_TDFN"
				(at 35.56 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max17260.pdf"
				(at 35.56 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "5.1µA 1-Cell Fuel Gauge with ModelGauge m5 EZ and Optional High-Side Current Sensing; T: -40 to 85°C"
				(at 35.56 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX17260SETD+"
				(at 35.56 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "PMIC, IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX17260_TDFN_1_1"
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TH")
					(number "1")
				)
				(pin no_connect line
					(at 2.54 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 2.54 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 2.54 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "BATT")
					(number "6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CSN")
					(number "7")
				)
				(pin power_in line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CSPL")
					(number "9")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "CSPH")
					(number "10")
				)
				(pin power_out line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "REG")
					(number "11")
				)
				(pin open_collector line
					(at 20.32 0 180)
					(length 2.54)
					(name "ALERT")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "SDA")
					(number "13")
				)
				(pin input line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin passive line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "EP")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
