(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX20087ATPA_VY+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX20087ATPA_VY+"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX20087ATPA_VY+"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/en/products/max20087.html"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual/Quad Camera Power Protector"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX20087ATPA/VY+"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, POWER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX20087ATPA_VY+_1_1"
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PGND")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IN")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "4")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "5")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "OUT1")
					(number "6")
				)
				(pin power_out line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "OUT3")
					(number "7")
				)
				(pin no_connect line
					(at 17.78 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin passive line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "ISET")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "11")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SDA")
					(number "13")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EN")
					(number "15")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "ADDR")
					(number "16")
				)
				(pin output line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "~{INT}")
					(number "17")
				)
				(pin no_connect line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "18")
				)
				(pin power_out line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "OUT4")
					(number "19")
				)
				(pin power_out line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "OUT2")
					(number "20")
				)
				(pin power_out line
					(at 0 -22.86 0)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
