(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX812REUS+T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX812REUS+T"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX812REUS+T"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX811-MAX812T.pdf"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Voltage monitor"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX812REUS+T"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, MONITOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX812REUS+T_1_1"
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "~{RST}")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{MR}")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
)
