(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX8902B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX8902B"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX8902B"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX8902-MAX8902B.pdf"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LDO Voltage Regulator, Adjustable, 1.7V to 5.5V input, 150 mV drop., 0.6-5.3V/0.5A out, TDFN-8"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX8902B"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX8902B_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin power_in line
					(at 15.24 -17.78 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin input line
					(at 15.24 -12.7 180)
					(length 2.54)
					(name "GS")
					(number "4")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{POK}")
					(number "5")
				)
				(pin input line
					(at 15.24 -8.89 180)
					(length 2.54)
					(name "FB")
					(number "6")
				)
				(pin input line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "BYP")
					(number "7")
				)
				(pin output line
					(at 15.24 0 180)
					(length 2.54)
					(name "OUT")
					(number "8")
				)
				(pin passive line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
