(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MIC2211-AAYML"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MIC2211-AAYML"
				(at 31.75 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MIC2211-AAYML"
				(at 31.75 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/mic2211.pdf"
				(at 31.75 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Linear voltage regulator"
				(at 31.75 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 31.75 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MIC2211-AAYML-TR"
				(at 31.75 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 31.75 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LDO, IC, LINEAR, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MIC2211-AAYML_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "1")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "EN_{1}")
					(number "2")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "EN_{2}")
					(number "3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 2.54)
					(name "BYP")
					(number "4")
				)
				(pin input line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "ADJ_{1}")
					(number "5")
				)
				(pin power_in line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin input line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "ADJ_{2}")
					(number "7")
				)
				(pin no_connect line
					(at 2.54 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin power_out line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "V_{OUT2}")
					(number "9")
				)
				(pin power_out line
					(at 17.78 0 180)
					(length 2.54)
					(name "V_{OUT1}")
					(number "10")
				)
				(pin power_in line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "EP")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
