(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MIC22705YML-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MIC22705YML-TR"
				(at 48.26 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MIC22705YML-TR"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/MIC22705_1MHz_7A_Integrated_Switch_High_Efficiency-1890923.pdf"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MIC22705YML-TR"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MIC22705YML-TR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PVIN")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN/DLY")
					(number "2")
				)
				(pin no_connect line
					(at 27.94 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RC")
					(number "4")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "PG")
					(number "5")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "7")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "8")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "9")
				)
				(pin power_out line
					(at 30.48 0 180)
					(length 2.54)
					(name "SW")
					(number "10")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "11")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PGND")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "13")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "FB")
					(number "14")
				)
				(pin input line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "COMP")
					(number "15")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SGND")
					(number "16")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SVIN")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "18")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "19")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "20")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "21")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "22")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "23")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "24")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "EP")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
