(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MP2386GG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MP2386GG"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MP2386GG"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2386GG-Z/document_id/4066/"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MP2386GG-P"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MP2386GG_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "1")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PGND")
					(number "2")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "3")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "4")
				)
				(pin open_collector line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "PG")
					(number "5")
				)
				(pin power_out line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "SW")
					(number "6")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "BST")
					(number "7")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AGND")
					(number "9")
				)
				(pin input line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "FB")
					(number "10")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
