(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MP8796B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MP8796B"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MP8796B"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP8796B/"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "16V, 30A, Scalable, Digital, Synchronous Step-Down Converter with PMBus"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MP8796BGVT-0000-Z"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Monolithic Power Systems"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, DC-DC, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MP8796B_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "2")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "3")
				)
				(pin passive line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "P_{GND}")
					(number "4")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "V_{DRV}")
					(number "5")
				)
				(pin open_collector line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin open_collector line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SDA")
					(number "7")
				)
				(pin open_collector line
					(at 0 -30.48 0)
					(length 2.54)
					(name "~{ALT}")
					(number "8")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "CTRL")
					(number "9")
				)
				(pin open_collector line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PG")
					(number "10")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PASS")
					(number "11")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TAKE")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SET")
					(number "13")
				)
				(pin power_in line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "P_{GND}")
					(number "14")
				)
				(pin passive line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "P_{GND}")
					(number "15")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "16")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "~{PS}")
					(number "17")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "ADDR")
					(number "18")
				)
				(pin passive line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "I_{SUM}")
					(number "19")
				)
				(pin passive line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "I_{REF}")
					(number "20")
				)
				(pin passive line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "V_{OSNS}-")
					(number "21")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "V_{OSNS}+")
					(number "22")
				)
				(pin power_in line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "A_{GND}")
					(number "23")
				)
				(pin power_out line
					(at 0 -20.32 0)
					(length 2.54)
					(name "V_{CC}")
					(number "24")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "BST")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
