(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NCP163ASN330T1G"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NCP163ASN330T1G"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NCP163ASN330T1G"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mouser.com/datasheet/2/308/1/NCP163_D-2317108.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fixed LDO Voltage Regulator, 2.2V to 5.5V, 105mV drop, 3.3V/250mA out, SOT-23-5"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NCP163ASN330T1G"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, LDO, VOLTAGE, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NCP163ASN330T1G_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "1")
				)
				(pin power_in line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin no_connect line
					(at 17.78 1.27 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "VOUT")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
