(footprint "SC-70-5"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "5-lead Small Outline SMT package (aka SC-70-5, SC-88A or TSSOP5): reflow soldering footprint")
	(tags "SOT-353 sot353 SC-70-5 sc70 SC-88A sc88a TSSOP5")
	(property "Reference" "REF**"
		(at 0 -1.6 180)
		(layer "F.SilkS")
	)
	(property "Value" "SC-70-5"
		(at 0 2.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.206 4.027 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.206 5.227 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.206 6.427 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.756 0.893 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.006 0.893 90)
		(size 0.6 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.743 0.893 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.743 -0.907 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.756 -0.907 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_ncp4683dsq33t1g.glb"
		(offset
			(xyz -0.005762 -0.035 0.71)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
