(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NCP718ASN500_SOT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NCP718ASN500_SOT"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NCP718ASN500_SOT"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/NCP718_D-1224359.pdf"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Linear Voltage Regulator IC Positive Fixed 1 Output 300mA TSOT-23-5"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NCP718ASN500T1G"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, LDO, VOLTAGE, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NCP718ASN500_SOT_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "1")
				)
				(pin power_in line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin no_connect line
					(at 12.7 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin power_out line
					(at 15.24 0 180)
					(length 2.54)
					(name "V_{OUT}")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
