(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PAC1720-1-AIA-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PAC1720-1-AIA-TR"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PAC1720-1-AIA-TR"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/PAC1710-PAC1720-Data-Sheet-DS20005386.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Current/Voltage Monitor Regulator High-Side VDFN-10 (3x3)"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PAC1720-1-AIA-TR"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MONITOR, VOLTAGE, IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PAC1720-1-AIA-TR_1_1"
				(pin input line
					(at 25.4 0 180)
					(length 2.54)
					(name "IN1+")
					(number "1")
				)
				(pin input line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "IN1-")
					(number "2")
				)
				(pin input line
					(at 25.4 -6.35 180)
					(length 2.54)
					(name "IN2+")
					(number "3")
				)
				(pin input line
					(at 25.4 -8.89 180)
					(length 2.54)
					(name "IN2-")
					(number "4")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "ADDRSEL")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{ALERT}")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SDA")
					(number "8")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SCL")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "10")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "EP")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
